=== Virtual COM Driver Installation Guide ===

The driver is for Win7 64bit, Win8 64bit PC.

Please follow the steps below to install virtual com driver.

1. Set PID/VID by scanning the sheet: TSCS161011-1(Omni)Set ST PID VID.pdf
2. Set virtual com by scanning the sheet: TSSOP121109-1(Omni)Set Virtual COM.pdf
3. Install the driver: VCP_V1.3.1_Setup_x64.exe


The default RS-232 parameters for scanner are:
ĦECOM Port Number = (check "Device Manager")
ĦEBaud Rate = 9600
ĦEData Bit = 8
ĦEStop Bit = 2
ĦEParity Check = None
ĦEHandshaking = None
ĦEDTR Check = Enable


